← All products
FIXED-MOUNT INTERACTION

# 13 inch Interactive Display

A rugged, fixed-mount touch display for visitor services, building information and exhibit interaction in shared environments.

FORM FACTOR 13 inch fixed-mount display
BEST FOR Visitor and building interaction
APPLICATIONS

## Information that invites interaction.

### Lift-car information

Floor navigation, building notices, lift calling and touch-operated fault reporting.

### Visitor registration

A durable reception touchpoint for self-registration and QR-code check-in.

### Exhibit interpretation

Touch-accessible content beside exhibits in museums, showrooms and visitor centres.

KEY SPECIFICATIONS

## Configured for connected installations.

  Display
    13 inch LCD with anti-glare / anti-fingerprint coating
  Resolution
    1920 × 1200
  Processor
    RockChip RK3576
  Memory / storage
    6 GB DDR5 / 64 GB UFS
  Network
    100 Mbit Ethernet; Wi-Fi and Bluetooth
  Interfaces
    RS485; USB-C with DisplayPort Alternate Mode
  Power
    USB-C or PoE
  Controls
    Bluetooth connection and volume buttons
  Enclosure
    Rugged plastic with customised mounting-plate area

PLANNED SOFTWARE & SECURITY SUPPORT

## Support planned through January 2030.

PM Plus plans to provide software and security maintenance for this model through the stated date. Contact Support with the model and serial number for the applicable release information and compatibility guidance.

PROJECT SUPPORT

## Planning a fixed installation?

Talk to PM Plus about mounting, power, network integration and support for your installed model.

Contact the team